; Jungo Confidential. Copyright (c) 2010 Jungo.  http://www.jungo.com
; Generated by DriverWizard v10.11.
; Installation file (.inf) for "MTC-610/611 Motion Control Card" device
;

[Version]
Signature="$CHICAGO$"  ; Represents all Windows OS's
Provider=%jun%
DriverVer=04/12/2010, 10.1.1

;Class=Jungo
;ClassGuid={c671678c-82c1-43f3-d700-0049433e9a4b}

Class=MCS
ClassGuid={E8B60D7E-0C35-4F84-A837-FC6C3C7BECCE}

; Driver Information
; ------------------
[Manufacturer]
%Mfg%=DeviceList,NTamd64


; x86 platform, Windows 2000 and later
[DeviceList]
"MTC-610/611 Motion Control Card"=Install, PCI\VEN_16A4&DEV_0611&SUBSYS_061116A4

; x64 platform, Windows XP x64 edition and later
[DeviceList.NTamd64]
"MTC-610/611 Motion Control Card"=Install, PCI\VEN_16A4&DEV_0611&SUBSYS_061116A4

; Installation Section
; --------------------
[Install.NT]  ; Installation script for Windows 2000 and later
CopyFiles=FilesToCopy
AddReg=UpDateRegistry

[FilesToCopy]
; To copy windrvr6.sys upon installation remove the ';' from the start of the following line
;windrvr6.sys ,,,0x40  ; 0x40 == COPYFLG_OVERWRITE_OLDER_ONLY

[ClassInstall32]  ; Register a new class in Windows 2000 and later
AddReg=UpDateRegistry

[UpDateRegistry]
HKR,,,,MCS
HKR,,Icon,,-5
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,, windrvr6.sys

[ControlFlags]
ExcludeFromSelect = *  

[PreCopySection]
HKR,,NoSetupUI,,1

; Defining WinDriver6 Service
; ---------------------------
[Install.NT.Services]
Addservice=WinDriver6, 0x00000002, Service_Info

[Service_Info]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\windrvr6.sys

; Source File Information
; -----------------------
[SourceDisksFiles]
windrvr6.sys=1  

[SourceDisksNames]
1="MCS Installation Disk",,  

[DestinationDirs]
DefaultDestDir=10, System32\Drivers  


;---------------------------------------------------------------;

[Strings]
jun="MCS"
Mfg="MCS"

